|  |  |  |
| --- | --- | --- |
|  | **ASSIGNMENT 4** | |
|  |  |  |
| **Date** |  | **27 October 2022** |
| **Team ID** |  | **PNT2022TMID53567** |
| **Project Name** |  | **Smart Waste Management** |
|  |  | **System for Metropolitan Cities** |

**QUESTION:**

**Write code and connections in wokwi for ultrasonic sensor. Whenever distance is less than 100 cms send "alert" to ibm cloud and display in device recent events.**

CODE:

#include <WiFi.h> #include <PubSubClient.h>

void callback(char\* subscribetopic, byte\* payload, unsigned int payloadLength);

//-------credentials of IBM Accounts------

#define ORG "u9pz01"//IBM ORGANITION ID #define DEVICE\_TYPE "ultrasensor"//Device type mentioned in ibm watson IOT Platform

#define DEVICE\_ID "123"//Device ID mentioned in ibm watson IOT Platform

#define TOKEN "12345678" //Token String data3;

char server[] = ORG

".messaging.internetofthings.ibmcloud.com";

char publishTopic[] = "iot-

2/evt/Data/fmt/json";

char subscribetopic[] = "iot-2/cmd/test/fmt/String";

char authMethod[] = "use-token-auth"; char token[] = TOKEN;

char clientId[] = "d:" ORG ":" DEVICE\_TYPE ":" DEVICE\_ID;

WiFiClient wifiClient;

PubSubClient client(server, 1883, callback ,wifiClient);

const int trigPin = 5; const int echoPin = 18; #define SOUND\_SPEED 0.034 long duration; float distance;

void setup() {

Serial.begin(115200);

pinMode(trigPin, OUTPUT);

pinMode(echoPin, INPUT);

wificonnect();

mqttconnect();

}

void loop()

{

digitalWrite(trigPin, LOW); delayMicroseconds(2); digitalWrite(trigPin, HIGH); delayMicroseconds(10); digitalWrite(trigPin, LOW); duration = pulseIn(echoPin, HIGH);

distance = duration \* SOUND\_SPEED/2;

Serial.print("Distance (cm): ");

Serial.println(distance);

if(distance<100)

{

Serial.println("ALERT!!");

delay(1000);

PublishData(distance);

delay(1000);

if (!client.loop()) {

mqttconnect();

}

}

delay(1000);

}

void PublishData(float dist) { mqttconnect();

String payload = "{\"Distance\":"; payload += dist;

payload += ",\"ALERT!!\":""\"Distance less

than 100cms\"";

payload += "}";

Serial.print("Sending payload: "); Serial.println(payload);

if (client.publish(publishTopic, (char\*)

payload.c\_str())) {

Serial.println("Publish ok");

} else {

Serial.println("Publish failed");

}

}

void mqttconnect() {

if (!client.connected()) {

Serial.print("Reconnecting client to "); Serial.println(server);

while (!!!client.connect(clientId, authMethod, token)) {

Serial.print(".");

delay(500);

}

initManagedDevice();

Serial.println();

}

}

void wificonnect()

{

Serial.println();

Serial.print("Connecting to "); WiFi.begin("Wokwi-GUEST", "", 6); while (WiFi.status() != WL\_CONNECTED) { delay(500);

Serial.print(".");

}

Serial.println("");

Serial.println("WiFi connected");

Serial.println("IP address: ");

Serial.println(WiFi.localIP());

}

void initManagedDevice() {

if (client.subscribe(subscribetopic)) { Serial.println((subscribetopic)); Serial.println("subscribe to cmd OK");

} else {

Serial.println("subscribe to cmd FAILED");

}

}

void callback(char\* subscribetopic, byte\* payload, unsigned int payloadLength) {

Serial.print("callback invoked for topic: "); Serial.println(subscribetopic);

for (int i = 0; i < payloadLength; i++) {

//Serial.print((char)payload[i]);

data3 += (char)payload[i];


}

Serial.println("data: "+ data3);


data3="";

}

**SCHEMATIC/CIRCUIT DIAGRAM:**

****

**IBM CLOUD OUTPUT:**



WOKWI LINK:

https://wokwi.com/projects/347241404309701203